Ladder Safety
[image: þÿ]Ladders are a commonly used piece of equipment both in the workplace and at home. Working with a ladder may seem straight forward enough, but before you begin your projects, take a few moments to review some safety tips that involve the use of ladders. A quick inspection now might keep you from being one of the estimated 200,000 people that are injured each year from falling off a ladder in the United States. Remember, most ladder deaths involve falls from less than 10 feet. The most important tip is to select the correct ladder for the job; it’s not a one-size fits all situation. No person ever plans to fall and it happens in an instant. Whether your task is cleaning gutters, hanging structural supports for a roof, or changing a light bulb, safe practices must be utilized in the set up and use of ladders.


Before You Climb:
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Read and follow all the manufacturer’s instructions and labels on the ladder.
Look for overhead electrical before handling or climbing a ladder.
Only put ladders on a stable and level surface that is not slippery.
Keep ladders free from any slippery material. Use a barricade to keep traffic away from the ladder.
Inspect for damaged parts (checklist attached). Check to make sure all components work.
Only use fiberglass ladders when working near electrical.
Position ladder to face work.
[image: In the 3-point system, a person climbing a ladder should always have 3 points of contact.]Fully open or extend ladder before starting to climb (extension ladder rails fully supported).














Safe Ladder Use—DO:
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Maintain a 3-point contact (two hands and a foot, or two feet and a hand).
Face the ladder while climbing or descending. Keep the body between the side rails.
Use extra care when getting on or off the ladder at the top or bottom.
Carry tools in a tool belt or raise tools up using a hand line. Never carry tools in your hands while climbing up/down a ladder.
Extend the top of extension ladders three feet above the landing.
Avoid tipping the ladder over sideways or causing the ladder base to slide out.
Wear shoes with non-slip soles.
Use extreme caution while pushing or pulling materials while on a ladder.
Always move one step at a time, never skip a step. Properly store ladders for protection from impact, heat, weather, and corrosive materials.
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Use a stepladder with spreaders unlocked.
Use ladders for a purpose other than that for which they were designed. For example, do not use a folded stepladder as a single ladder.
Use a ladder horizontally like a platform. Leave tools/materials/equipment on stepladder.
Move or shift a ladder with a person or equipment on the ladder (descend and reposition).
Use cross bracing on the rear of stepladders for climbing. Stand above the second step from the top of a stepladder or the forth rung from the top of an extension ladder.
Paint a ladder with opaque coatings. Sit on a step ladder top cap.
Use a damaged ladder.
Place a ladder on boxes, barrels, or unstable bases. Exceed the ladder’s maximum load rating.
Tie two ladders together to make them longer. Ignore nearby overhead electrical.
Lean out beyond the ladder’s side rails.
Use metal or wood ladders when working near electricity. Climb a closed stepladder.
Use a ladder if you are injured.
Place an extension ladder too far or close to the building. (Maintain 4:1 ratio; set back is one foot for each four feet of length to upper support point).









State of Wisconsin, Bureau of State Risk Management
Sources: OSHA


Additional Reference:
-OSHA Extension Ladder Fact Sheet
-OSHA Stepladder Fact Sheet
-Stairways and Ladders Guide to OSHA Rules
-DOA Slip, Trip, Fall Prevention Manual
-Ladder Training Resource
-Podium Ladder Example

Ladder Inspection Checklist

	Inspector:
	Date:

	Ladder ID Number:
	Assigned Location/Department:

	Type of Ladder:

	If a ladder is determined to be defective it shall be removed from service immediately, marked with a tag reading “DANGEROUS – DO NOT USE” The
Environmental Health & Safety Office shall be notified.

	Ladder is free of sharp edges, splinters, cracks, slivers, or dents that would compromise structural integrity.
	· Yes
	· No
	· NA

	Joints between the steps/rungs and sides must be tight. Rungs should not move when twisted by hand.
	· Yes
	· No
	· NA

	Hardware and fittings are securely attached.
	· Yes
	· No
	· NA

	Moveable parts operate freely (lubricate, if necessary), but without undue play.
	· Yes
	· No
	· NA

	Safety feet/pads are non-slip, insulated, in place and unbroken.
	· Yes
	· No
	· NA

	Rungs/steps are free of grease, oil, or other slippery substances. Remove any buildup of dirt or mud, as well. Rungs must be corrugated, knurled, dimpled, or coated with a slip-resistant
material.
	· Yes
	· No
	· NA

	No rungs/steps are missing or defective.
	· Yes
	· No
	· NA

	Ladder is not painted or coated with any material that might hide defects. Labels should be placed on only one face of side
rails.
	· Yes
	· No
	· NA

	Step ladders must have a metal spreader or locking device of sufficient size and strength to securely hold the ladder in an open position. Any sharp points on the spreader must be
covered or removed.
	· Yes
	· No
	· NA

	Mobile ladders with a working platform have protected toe guards, top, and mid-rails.
	· Yes
	· No
	· NA

	Is the ladder free from any other defects that may impair its safe usage.
	· Yes
	· No
	· NA


Ladder Disposal Date:
Comments:
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